Perhaps start by seeing if you can run the instructions already implemented

See mips-control.v. To add signals, figure out their opcode and add them to the case statement path. Set the control signals accordingly. You may need to add more control signals later. Start by implementing add: set the control signals